#### NIFF 1.0 Specification

## 3. Binary Format

### 3.11 TriList

#### 4) ReferenceTriColorData Area

When TRI_ANIM_TRI_COLOR_FULL is specified

u32 | tri_color_group_index(0)
...
u32 | tri_color_group_index(tri_anim_frame_num)

Reference TriColorData Area Memory Map

u32 tri_color_group_index | Index number of TriColorGroup to be referred

When TRI_ANIM_TRI_COLOR_KEY is specified

u32 | tri_color_anim_key_num
u32 | tri_color_anim_key(0)
...
u32 | tri_color_anim_key(tri_color_anim_key_num - 1)
u32 | tri_color_group_index(0)
...
u32 | tri_color_group_index(tri_color_anim_key_num - 1)

Reference TriColorData Area Memory Map

u32 tri_color_anim_key_num | Total number of key frame animation keys.
u32 tri_color_anim_key | Key frame value
u32 tri_color_group_index | Index number of TriColorGroup to be referred

When Tri Color Animation is not performed

u32 | tri_color_group_index

ReferenceTriColorData Area Memory Map

u32 tri_color_group_index | Index number of TriColorGroup to be referenced

Copyright 1997-1999 NINTENDO Co., Ltd. All rights reserved.