Function

    nuContRmbSearchTimeSet

    Syntax:

    void nuContRmbSearchTimeSet(u32 frame)

    Arguments:

    fame	The time period between checks (in frames)

    Return Value:

    None

    Explanation:

Sets the time for checking the Rumble Pak

When the NU_CONT_RMB_MODE_AUTO mode has been set with the nuContRmbModeSet function, this function specifies the time (in frames) between each check to see whether the Rumble Pak is inserted. The default value is set at 300 frames (5 seconds). The Rumble Pak Manager does not check all four Controllers during the same frame, so the burden of checking does not fall all at once.

    Reference:	nuContRmbModeSet