Function 
(  Provides input stream from ROM which uses PI manager. 

Functions 
(  void misRomInputPiInit( MisRomInputPi *rom_input_ptr )
  Initializes misRomInput. 

(  void misRomInputPiOpen( MisRomInputPi *rom_input_ptr, const u32 dev_addr,
			const u32 size )
  Opens misRomInputPi.  Device address at head of load is specified by dev_address and size is specified 
  by size (number of bytes). 

NOTE 
*  Cast from MisRomInputPi * to MisInput * as follows: 
   input_ptr = _msoUpCast( MisInput, rom_input_ptr );

History 
  1998/ 9/24 Takamitsu Hirata 
    RomInputPi.h, rominputpi.c :  Initial version 
