#### NIFF 1.0 Specification

## 3. Binary Format

### 3.18 CamList

#### 1) CamList Area

> The CamList area describes data related to the camera node. The mapping for CamList is as follows.

CamListHeader | u32 | cam_list_tag
u32 | cam_list_header_size
u32 | cam_list_size
u32 | cam_num
u32 | nintendo_extension_block_size
u32 | user_extension_block_size
u32 | cam_num_byte(0)
...
u32 | cam_num_byte(cam_num - 1)
| Cam(0)
...
Cam(cam_num - 1)
NintedoExtensionBlock
UserExtensionBlock

CamList Area Memory Map

u32 cam_list_tag | Tag indicating CamList
    TAG_CAM_LIST    0x000e0000
u32 cam_list_header_size | Size of CamListHeader
u32 cam_list_size | Size of CamList
u32 cam_num | Total number of Cam in CamList
u32 nintendo_extension_block_size | Nintendo extension block size
u32 user_extension_block_size | User extension block size
u32 u32 cam_num_byte | Number of bytes corresponding to Cam
Cam | Actual camera data
NintendoExtensionBlock | Nintendo extension block
UserExtensionBlock | User extension block

Copyright 1997-1999 NINTENDO Co., Ltd. All rights reserved.