Clock Speeds and Bus Bandwidth

Various system statistics and bandwidths:

- CPU - 94.0 Mhz

- RDRAM - 250 Mhz (9 bit bytes at 500 M/sec)

- RCP - 62.6 Mhz

- AI - variable, 3000-368000hz on NTSC, 3050-376000 on PAL

- VI - (depends on mode) NTSC, PAL, MPAL

- PI - 20 Meg/sec peak, 5 Meg/sec from typical slow ROMs

- SI - very slow

Copyright © 1999 Nintendo of America Inc. All Rights Reserved Nintendo and N64 are registered trademarks of Nintendo Last Updated January, 1999