N64® Functions Menu

al - Audio Library Functions
gDP - DP GBI Macros
gdSP - General GBI Macros
gSP - SP GBI Macros
gt - Turbo Microcode RDP
gu - Graphics Utilities
Math - Math Functions
nuSys - NuSystem
os - N64 Operating System
sp - Sprite Library Functions
uh - Host to Target IO
64DD - N64 Disk Drive

Nintendo® Confidential

## alCSeqPlayer

Syntax

    #include <libaudio.h>

    void    alCSPNew(ALCSPlayer *seqp, ALSeqpConfig *config);

    void    alCSPDelete(ALCSPlayer *seqp);

    void    alCSPSetSeq(ALCSPlayer *seqp, ALCSeq *seq);

    ALCSeq  *alCSPGetSeq(ALCSPlayer *seqp);

    void    alCSPSetBank(ALCSPlayer *seqp, ALBank *b);

    s32     alCSPGetState(ALCSPlayer *seqp);

    void    alCSPPlay(ALCSPlayer *seqp);

    void    alCSPStop(ALCSPlayer *seqp);

    void    alCSPSetBank(ALCSPlayer *seqp, ALBank *b);

    void    alCSPSetTempo(ALCSPlayer *seqp, s32 tempo);

    s32     alCSPGetTempo(ALCSPlayer *seqp);

    s16     alCSPGetVol(ALCSPlayer *seqp);

    void    alCSPSetVol(ALCSPlayer *seqp, s16 vol);

    void    alCSPSetChlProgram(ALCSPlayer *seqp, u8 chan, u8 prog);

    s32     alCSPGetChlProgram(ALCSPlayer *seqp, u8 chan);

    void    alCSPSetChlFXMix(ALCSPlayer *seqp, u8 chan, u8 fxmix);

    u8      alCSPGetChlFXMix(ALCSPlayer *seqp, u8 chan);

    void    alCSPSetChlPan(ALCSPlayer *seqp, u8 chan, ALPan pan);

    ALPan   alCSPGetChlPan(ALCSPlayer *seqp, u8 chan);

    void    alCSPSetChlVol(ALCSPlayer *seqp, u8 chan, u8 vol);

    u8      alCSPGetChlVol(ALCSPlayer *seqp, u8 chan);

    void    alCSPSetChlPriority(ALCSPlayer *seqp, u8 chan, u8 priority);

    u8      alCSPGetChlPriority(ALCSPlayer *seqp, u8 chan);

    void    alCSPSendMidi(ALCSPlayer *seqp, long ticks, u8 status, u8
    byte1, u8 byte2);

Explanation
The Nintendo 64 Audio Library supports the playback of MIDI sequences using either the Type 0 MIDI Sequence Player (function names that begin with alSeqp) or the Compressed MIDI Sequence Player (function names that begin with alCSP).
This page details the Compressed MIDI Sequence Player. For details about the Type 0 MIDI Sequence Player, see the alSeqPlayer page.
The principle differences between the two MIDI players are the handling of loops, and the compression of data. Details are discussed in the Audio Library and Audio Formats sections of the Nintendo 64 Programming Manual.
The sequence player handles the playback of the sequence, but the actual sequence data is handled by a Sequence (see alCSeq).
To use a Compressed Sequence Player, you must first initialize an ALCSPlayer structure to represent it. This is accomplished by calling the alCSPNew function.
After initializing the ALCSPlayer structure, you must set the bank and the sequence by calling alCSPSetBank and alCSPSetSeq respectively.
To start the sequence player, call alCSPPlay. To stop the sequence player, call alCSPStop. The sequence player can only have one target sequence at a time. You must stop a sequence before setting and playing a new sequence. You should not attempt to switch banks while a sequence is playing. You can use alCSPGetSeq to determine if the sequence player is fully stopped. When you call alCSPStop, all processing of the sequence will stop and all notes will be turned off.
When a sequence is stopped, it will not rewind; it continues to point to its current location. This allows you to restart a sequence from where it was stopped by calling alCSPPlay. Sustained notes that were cut off by a call to alCSPStop are not restarted, only new notes are processed.
If you want to rewind the sequence or relocate to another point in the sequence, you can create an ALCSeqMarker at the desired location by calling the alCSeqNewMarker function. Then call alCSeqSetLoc to rewind or relocate the sequence. Note that these calls do not affect the channel playback state, so you must ensure that the channel arguments (such as program, volume, pan, and so on) are set to appropriate values for the given sequence location.
Channel arguments can be set by calling their individual functions or by sending the appropriate midi data using the alCSPSendMidi function. Music can be created in real time and played back by calling the alCSPSendMidi
function.
The compressed MIDI sequence player does not support loops created by application programming interface (API) calls. However, the Type 0 MIDI sequence player does. To loop music using the compressed MIDI sequence player, you must ensure that the sequences have loop points embedded in them. To learn how to embed loop points, see the Audio Library section of the Nintendo 64 Programming Manual.
See Also
alCSeq
alCSPNew
alCSPDelete
alCSPSetSeq
alCSPGetSeq
alCSPPlay
alCSPStop
alCSPSetBank
alCSPSetTempo
alCSPGetTempo
alCSPGetVol
alCSPSetVol
alCSPSetChlProgram
alCSPGetChlProgram
alCSPSetChlFXMix
alCSPGetChlFXMix
alCSPSetChlPan
alCSPGetChlPan
alCSPSetChlVol
alCSPGetChlVol
alCSPSetChlPriority
alCSPGetChlPriority
alCSPSendMidi

Nintendo® Confidential Warning: all information in this document is confidential and covered by a non-disclosure agreement. You are responsible for keeping this information confidential and protected. Nintendo will vigorously enforce this responsibility.
Copyright © 1998
Nintendo of America Inc. All rights reserved
Nintendo and N64 are registered trademarks of Nintendo
Last Updated April, 1999