N64® Functions Menu

al - Audio Library Functions
gDP - DP GBI Macros
gdSP - General GBI Macros
gSP - SP GBI Macros
gt - Turbo Microcode RDP
gu - Graphics Utilities
Math - Math Functions
nuSys - NuSystem
os - N64 Operating System
sp - Sprite Library Functions
uh - Host to Target IO
64DD - N64 Disk Drive

Nintendo® Confidential

## osAiGetLength

Syntax
#include <ultra64.h>
u32 osAiGetLength(void);
Explanation
The osAiGetStatus, osAiGetLength, osAiSetFrequency, and osAiSetNextBuffer routines provide basic control for the AI (audio interface).
This function (osAiGetLength) returns the number of bytes remaining in the current DMA buffer.
Notes
For hardware version 1.0, the audio DMA length register is only 15-bit long and thus supports a maximum transfer size of 32 Kbytes. In the final release, this register is extended to 18 bits to support a transfer of 256 Kbytes.
See Also
osAiGetStatus
osAiSetFrequency
osAiSetNextBuffer
osTvType

Nintendo® Confidential Warning: all information in this document is confidential and covered by a non-disclosure agreement. You are responsible for keeping this information confidential and protected. Nintendo will vigorously enforce this responsibility.
Copyright © 1998
Nintendo of America Inc. All rights reserved
Nintendo and N64 are registered trademarks of Nintendo
Last updated March 1998