N64® Functions Menu

al - Audio Library Functions
gDP - DP GBI Macros
gdSP - General GBI Macros
gSP - SP GBI Macros
gt - Turbo Microcode RDP
gu - Graphics Utilities
Math - Math Functions
nuSys - NuSystem
os - N64 Operating System
sp - Sprite Library Functions
uh - Host to Target IO
64DD - N64 Disk Drive

Nintendo® Confidential

## alCSPGetChlFXMix

Syntax

    #include <libaudio.h>
    u8 alCSPGetChlFXMix(ALCSPlayer *seqp, u8 chan);

Arguments

- seqp is the pointer to compressed MIDI sequence player
- chan is the target (0 based) MIDI channel

Explanation
It returns the effect mix for the given MIDI channel. A value of 0 indicates that the sound is completely dry, and 127 indicates the sound is completely wet. Because messages generated by the alCSPSetChlFXMix function are not processed until the next call to alAudioFrame, a call to alCSPSetChlFXMix followed by a call to alCSPGetChlFXMix within the same frame will not reflect the new value.
See Also
alCSPSetChlFXMix
alCSeqPlayer

Nintendo® Confidential Warning: all information in this document is confidential and covered by a non-disclosure agreement. You are responsible for keeping this information confidential and protected. Nintendo will vigorously enforce this responsibility.
Copyright © 1998
Nintendo of America Inc. All rights reserved
Nintendo and N64 are registered trademarks of Nintendo
Last Updated April, 1999