Function

    nuVrsOpen

    Syntax:

    s32 nuVrsOpen(NUVrsHandle* handle, s32 contNo)

    Arguments:

    handle  NUVrsHandle structure
    contNo  Controller No.

    Return Value:

    Error

    Description:

Initializes Voice Recognition System

Initializes the Voice Recognition System by calling the osVoiceInit function.

The return value is the return value from the osVoiceInit function.

This function calls the osVoiceInit function via the SI manager.

Errors:

CONT_ERR_NO_CONTROLLER | Nothing is connected to the Controller port.
CONT_ERR_DEVICE | Something other than the Voice Recognition System is connected to the Controller port.
CONT_ERR_VOICE_NO_RESPONSE | No response from Voice Recognition System. There may be a problem with the hardware.
CONT_ERR_CONTRFAIL | Data transfer failure. There is a problem in the Voice Recognition System connection.
CONT_ERR_INVALID | There is an error in the way this function was called or in the argument. This error will not occur if the correct calling method is used. Please correct the error so that this error does not occur when development is completed.