#### NIFF 1.0 Specification

## 3. Binary Format

### 3.22 NameList

#### 2) Name Area

> The Name area stores the actual node Name. The Name area is mapped as follows.

NameHeader | u32 | name_tag
u32 | this_name_index
u32 | name_header_size
u32 | name_size
| node_name

Name Area Memory Map

u32 name_tag | Tag indicating Name
    TAG_NAME        0x00110100
u32 this_name_index | Index number of this Name
u32 name_header_size | Size of this NameHeader
u32 name_size | Size of this Name
node_name | Node name*

> *Note: The node name is entered as ASCII text. Permissible ASCII characters are 0x21 (!) through 0x7e (~), in ASCII code. If the number of characters is not a multiple of 4 bytes, embed NULL bits to make the number of characters a multiple of 4 bytes. If the character string count is a multiple of 4 bytes, there is no need to insert NULL bits.

Copyright 1997-1999 NINTENDO Co., Ltd. All rights reserved.