Function

    nuVrsStopReadData

    Syntax:

    s32 nuVrsStopReadData(NUVrsHandle* handle)

    Argument:

    handle   NUVrsHandle structure

    Return Value:

    Error

    Description:

Forces termination of recognition processing

This forcibly terminates voice recognition processing.

"handle" must be initialized with the nuVrsOpen function. The return value is the return value from the osVoiceStopReadData function.

This function calls the osVoiceStopReadData function via the SI manager.

Errors:

CONT_ERR_NO_CONTROLLER | Nothing is connected to the Controller port.
CONT_ERR_DEVICE | Something other than the Voice Recognition System is connected to the Controller port.
CONT_ERR_VOICE_NO_RESPONSE | No response from Voice Recognition System. There may be a problem with the hardware.
CONT_ERR_CONTRFAIL | Data transfer failure. There is a problem in the Voice Recognition System connection.
CONT_ERR_INVALID | There is an error in the way this function was called or in the argument. This error will not occur if the correct calling method is used. Please correct the problem so that this error does not occur when development is completed.

Reference: nuVrsOpen, osVoiceStopReadData