N64® Functions Menu

al - Audio Library Functions
gDP - DP GBI Macros
gdSP - General GBI Macros
gSP - SP GBI Macros
gt - Turbo Microcode RDP
gu - Graphics Utilities
Math - Math Functions
nuSys - NuSystem
os - N64 Operating System
sp - Sprite Library Functions
uh - Host to Target IO
64DD - N64 Disk Drive

Nintendo® Confidential

## threadstatus

Syntax

    threadstatus thread

Explanation
It displays the status of a target system thread. Specifically, it sends a message asking for the status of the specified thread running on the target system by using the dbgif tool and displays the result of the command on stdout.
Before executing this command, ensure that the dbgif program is running and the METHOD environment variable has been set to indicate if this is a request for the R4300 CPU or the coprocessor. The value zero represents the CPU and the number one represents the RCP. In csh, this is accomplished by specifying:

    setenv METHOD 0

Bugs
In the event of a communications failure, the program dumps core, which must be removed manually.
See Also
dbgif
listthreads

Nintendo® Confidential Warning: all information in this document is confidential and covered by a non-disclosure agreement. You are responsible for keeping this information confidential and protected. Nintendo will vigorously enforce this responsibility.
Copyright © 1998
Nintendo of America Inc. All rights reserved
Nintendo and N64 are registered trademarks of Nintendo
Last updated March 1998