     Global Variables

    nuAuDmaBufSize
    nuAuDmaBufNum

Syntax

    s16 nuAuDmaBufSize
    s16 nuAuDmaBufNum

Explanation
Size and number of audio PI-DMA buffers.

The number of DMA buffers specified by nuAuDmaBufNum of the size specified by nuAuDmaBufSize are reserved from the audio heap by the nuAuDmaNew function.

These DMA buffers are used when transferring waveform data requested from the synthesizer driver.
These are also used as waveform data caches which hold data for several frames (the default is one frame).

As a default, nuAuDmaBufSize and nuAdDmaBufNum are defined as NU_AU_DMA_BUFFER_SIZE and NU_AU_DMA_BUFFER_NUM, which are 1024 bytes and 64, respectively.

When audio cannot be played back well with these values, set these variables to suitable values.

When these variables are changed, set the values before calling the following functions:

nuAuInit
nuAuInitEx
nuAuMgrInit
nuAuMgrInitEx