## 第3章　バイナリフォーマット

### 3-11. TriList

#### (9)Triエリア

u32 | tri_tag
u32 | this_tri_index
u32 | tri_size
u32 | tri_nv_index
u32 | tri_color_index
u32 | vtx_index0
u32 | st_index0
u32 | vtx_nv_index0
u32 | vtx_color_index0
u32 | vtx_index1
u32 | st_index1
u32 | vtx_nv_index1
u32 | vtx_color_index1
u32 | vtx_index2
u32 | st_index2
u32 | vtx_nv_index2
u32 | vtx_color_index2
u32 | nintendo_extension_block_size
u32 | user_extension_block_size
NintendoExtensionBlock
UserExtensionBlock

図　Triエリアメモリマップ

u32 tri_tag | Tri indicated tag, specify the following tag
    TAG_TRI 0x00080101
u32 this_tri_index | Index number of this Tri area
u32 tri_size | Number of bytes of this Tri area
u32 tri_nv_index | Index number of TriNv contained in the TriNvGroup to be referred
u32 tri_color_index | Index number of TriColor in the TriColorGroup to be referred
u32 vtx_index0 | Index of Vtx contained in the VtxGroup to be referred. Specify three point for drawing triangle.
u32 st_index0 | Index number of St contained in this StGroup
u32 vtx_nv_index0 | Index number of VtxNv contained in the VtnNvGroup to be referred
u32 vtx_color_index0 | Index number of VtcColor contained in the VtxColorGroup to be referred
u32 vtx_index1 | Index number of Vtx to be referred
u32 st_index1 | Index number of St to be referred
u32 vtx_nv_index1 | Index number of VtxNv to be referred
u32 vtx_color_index1 | 参照するVtxColorのインデックス番号
u32 vtx_index2 | 参照するVtxのインデックス番号
u32 st_index2 | 参照するStのインデックス番号
u32 vtx_nv_index2 | 参照するVtxNvのインデックス番号
u32 vtx_color_index2 | 参照するVtxColorのインデックス番号
u32 nintendo_extension_block_size | 任天堂拡張ブロックサイズ
u32 user_extensino_block_size | ユーザー拡張ブロックサイズ
NintendoExtensionBlock | 任天堂拡張ブロック
UserExtensinoBlock | ユーザー拡張ブロック

Copyright 1997 NINTENDO Co.,Ltd. All rights reserved.

目次へ次へ