    Function

    nuAuSeqPlayerGetChlPriority (Macro)

Syntax

    u8 nuAuSeqPlayerGetChlPriority(u32 player_no, u8 chan)

Arguments

- player_no is the sequence player number

- chan is the MIDI channel

Return Value
Priority (0-127)

Explanation
Obtain the priority order for the MIDI channel specified by the player which is specified by sequence player number. The lowest priority value is 0 and the highest priority value is 127.

See Also
alCSPGetChlPriority