# 3.9.1 Display List Control

## GBI Commands

gSPSegment - Set the segment register and base address.
gSPBranchLessZ - Process the model's LOD.
gSPBranchList - Branch the display list.
gSPDisplayList - Branch execution with the current display list.
gSPEndDisplayList - Terminate the display list command.
gSPLoadUcode - Load specified microcode.
gSPLoadUcodeL - Load specified microcode.
gDPPipeSync - Synchronize the RDP attribute change which is on the primitive drawing.
gDPFullSync - Signal the end of a frame.
gDPLoadSync - Synchronize the texture load which is on the primitive drawing.
gDPTileSync - Synchronize the texture tile change which is on the primitive drawing.

Nintendo® Confidential
Copyright © 1999
Nintendo of America Inc. All Rights Reserved
Nintendo and N64 are registered trademarks of Nintendo
Last Updated March, 1999