# mfsSetRtc

Format

  s32 mfsSetRTC(LEODiskTime* time)

Arguments

  time LEODiskTime structure buffer

Return value

  Error

Function

  Sets internal RTC

Description

This function sets the date and time of the internal RTC to the values specified by time. It enables LeoSetRTC to be handled by using the MFS library.

Main errors

  MFS_ERR_NO
  Normal termination
  MFS_ERR_DEVICE
  Device error
  An error occurred in an internally called Leo function. Since a Leo function error is stored in the variable mfsError, check this variable to perform processing.