N64® Functions Menu

al - Audio Library Functions
gDP - DP GBI Macros
gdSP - General GBI Macros
gSP - SP GBI Macros
gt - Turbo Microcode RDP
gu - Graphics Utilities
Math - Math Functions
nuSys - NuSystem
os - N64 Operating System
sp - Sprite Library Functions
uh - Host to Target IO
64DD - N64 Disk Drive

Nintendo® Confidential

## osAfterPreNMI

Initializes the RSP's program counter (PC).

Syntax
#include <ultra64.h>
s32 osAfterPreNMI(void);

Explanation
The application will call this function every time after it receives a pre-NMI or after all RSP tasks have been completed.

A 0 is returned if the function is called successfully. When the RSP is running, a -1 is returned if the call fails. In the event of a failure, wait for the RSP task currently running to finish, then call the function again.

Nintendo® Confidential Warning: all information in this document is confidential and covered by a non-disclosure agreement. You are responsible for keeping this information confidential and protected. Nintendo will vigorously enforce this responsibility.
Copyright © 1998
Nintendo of America Inc. All rights reserved
Nintendo and N64 are registered trademarks of Nintendo
Last updated March 1998