Event and Interrupt Functions

- osSetEventMesg
  This function call specifies a message queue and message to be sent in response to a system event.

- osGetIntMask This function returns the current interrupt mask (including both the R4300 and RCP masks).

- osSetIntMask
  This function specifies a new interrupt mask (including both the R4300 and RCP masks).

Copyright © 1999 Nintendo of America Inc. All Rights Reserved Nintendo and N64 are registered trademarks of Nintendo Last Updated January, 1999