# mfsHResetVolumeRC

Format: s32 mfsHResetVolumeRC(s32 drive)

Arguments:

drive Drive name ('A', 'B', ...)

Return value:Error

Function: Resets update counter of volume

Description: This function resets the update counter value of the volume to 0. Since the update counter only exists in the RAM area, the MFS_ERR_REFUSE error will occur if this function is used for the ROM area.

Main errors:

    MFS_ERR_NO		Normal termination
    MFS_ERR_NOTFOUND	Drive not found
    MFS_ERR_DEVICE		Device error
    			An error occurred in an internally called Leo function.
    Since a Leo function error is stored in the variable mfsError, check this variable to perform processing.
    MFS_ERR_PROTECT		Write protected
    			The volume attribute is write protected, or the medium is volume protected.
    MFS_ERR_REFUSE 		Illegal operation