Function

    nuContDataGet

    Syntax:

    void nuContDataGet(OSContPad *contpad, u32 cont_no)

    Arguments:

    *contpad	 Controller data structure
    cont_no		 The number of Controller read

    Return Value:

    None

    Explanation:

Gets the Controller data

The Controller data is read at retrace time, or with the osContDataRead function, and stored in the internal buffer of the Controller Manager. The nuContDataGet function copies the data from the internal buffer. To get data from all 4 controllers, please use nuContDataGetAll.

    For Example:
    	OSContPad	padData;

    	/* read data from 1 Controller */
    	nuContDataGet(&padData, 0);

Note:

This function was a macro in V1.1

    Reference: nuContDataRead,nuContDataGetAll