Microcode in Alphabetical Order Nintendo® Confidential

To search the list, choose Find from the Edit menu in your browser.

gspF3DEX | Part of the F3DEX microcode series
gspF3DLP.Rej | Part of the F3DEX microcode series
gspF3DLX | Part of the F3DEX microcode series
gspF3DLX.Rej | Part of the F3DEX microcode series
gspFast3D | High quality 3D polygonal geometry RSP microcode
gspL3DEX | Part of the F3DEX microcode series
gspLine3D | High quality 3D line RSP microcode
gspS2DEX | Microcode that uses Super NES-like sprite and BG functions on the N64 to make it easier to create a game using sprites; it makes N64 programming similar to conventional sprite game programming
gspSprite2D | High-quality 2D sprite geometry microcode
gspTurbo3D | Reduced-feature, reduced-precision microcode that delivers significantly faster performance
Introduction to N64 Microcode | Introduces the seven basic microcodes and the F3DEX microcode series
rspboot | Microcode that enforces the OS synchronization between the host CPU (R4300) and the RSP. It processes the task header structure, loads the microcode for the task, and begins the task execution. The boot code does not remain in IMEM, so it is re-loaded at the beginning of each task

Warning: all information in this document is confidential and covered by a non-disclosure agreement. You are responsible for keeping this information confidential and protected. Nintendo will vigorously enforce this responsibility. Copyright © 1998
Nintendo of America Inc.
All rights reserved.
Last updated March 1998