N64® Functions Menu

al - Audio Library Functions
gDP - DP GBI Macros
gdSP - General GBI Macros
gSP - SP GBI Macros
gt - Turbo Microcode RDP
gu - Graphics Utilities
Math - Math Functions
nuSys - NuSystem
os - N64 Operating System
sp - Sprite Library Functions
uh - Host to Target IO
64DD - N64 Disk Drive

Nintendo® Confidential

## guMtxCatF

Syntax

    #include "gu.h"

    void guMtxCatF(float mf[4][4],
       float nf[4][4], float resf[4][4])

Arguments

- mf is the first 4x4 matrix

- nf is the second 4x4 matrix

- resf is the resulting 4x4 matrix, mf*nf

Explanation
It concatenates two 4x4 floating point matrices. This function is useful for matrix processing on the host CPU. It performs a 4x4 matrix multiplication of two matrices. The result is allowed to be one of the inputs.
See Also
guMtxCatL

Nintendo® Confidential Warning: all information in this document is confidential and covered by a non-disclosure agreement. You are responsible for keeping this information confidential and protected. Nintendo will vigorously enforce this responsibility.
Copyright © 1998
Nintendo of America Inc. All rights reserved
Nintendo and N64 are registered trademarks of Nintendo
Last Updated April, 1999