    Function

    nuAuStlPtrBankSet

    Syntax:

    void nuAuStlPtrBankSet(u8 *pbk_addr, u32 pbk_size, u8 *wbk_addr)

    Arguments:

    pbk_addr        ROM address of sample pointer bank
    pbk_size        Size of sample pointer bank
    wbk_addr        ROM address of sample wave bank

    Return Value:

    None

    Description:

Reads and initializes the sample pointer bank. Then makes associations with the sample wave bank and registers it in the mus library.