    Function

    nuAuSeqPlayerSetChlPriority (Macro)

Syntax

    void nuAuSeqPlayerSetChlPriority(u32 player_no, u8 chan, u8 priority)

Arguments

- player_no is the sequence player number

- chan is the object for MIDI channel number

- priority is the priority order for MIDI channel (0-127)

Return Value
None

Explanation
Set a priority order for the MIDI channel specified by the player which is specified by sequence player number. The lowest priority is a value of 0 and the highest priority is a value of 127.

See Alsp
alCSPSetChlPriority