     Global Variables

    nuAuDebugFlag

Syntax

    u32 nuAuDebugFlag

Explanation
Debug Flags

This enables the debugging function specified to the audio manager while debugging or tuning audio.

The values which can be specified are as follows. When multiple are specified, they can be specified using "or".

NU_AU_DEBUG_NORMAL | Performs warning or error output. Output is sent to the console by the osSyncPrintf function.
NU_AU_DEBUG_DISABLEDMA | Prohibits PI-DMA transfer
NU_AU_DEBUG_DISABLEAI | Prohibits setting an audio buffer in the AI register
NU_AU_DEBUG_DISABLETASK | Prohibits execution of audio tasks
NU_AU_DEBUG_FIFOOFF | Disables FIFO events
NU_AU_DEBUG_RETRACEOFF | Disables retrace events