# mfsRamSetDestination

    Format:	s32 mfsRamSetDestination(u8 destination)
    Arguments:	destination	Destination code
    Return value:Error
    Function:	Sets destination code
    Description:	This function sets the destination code.
    	The following values can be set for destination.

    		MFS_DESTINATION_JAPAN	0	Japan-oriented
    		MFS_DESTINATION_US	1	US-oriented

    	Since the destination code is set when the volume is formatted, normally this function should not be used.

    Main errors:
    	MFS_ERR_NO	Normal termination
    	MFS_ERR_NOTMFSDISK	Not an MFS-format disk
    			The disk ID's disk use is not 1, or the header is different.
    	MFS_ERR_VERSION	Different version MFS-format disk
    			The version is an unsupported version.
    	MFS_ERR_PROTECT	Write protected
    			The medium is volume protected.