N64® Functions Menu

al - Audio Library Functions
gDP - DP GBI Macros
gdSP - General GBI Macros
gSP - SP GBI Macros
gt - Turbo Microcode RDP
gu - Graphics Utilities
Math - Math Functions
nuSys - NuSystem
os - N64 Operating System
sp - Sprite Library Functions
uh - Host to Target IO
64DD - N64 Disk Drive

Nintendo® Confidential

## ginv

###

###

###

###

    README_DEMOS CONTENTS:
    	A simple hardware inventory app that reports which version
    	of the RCP is on the current development board, the speed
    	of the RCP and CPU, amount of DRAM available, etc...

    README CONTENTS:
    	n/a

    DESCRIPTION:
    	Screen display
    		RELEASE 2.0
    		RCP Version 2.0
    		PIF Version 1
    		DRAM size 4194304 bytes
    		System Clock Ratio = 3:2
    		R4300 freq = 94.0 Mhz
    		RCP freq = 62.6 Mhz
    		Video Mode is NTSC
    		ROM base address of the game image is 0xb0000000
    		ROM type is cartridge
    		Reset type is cold reset

    CONTROLLER FUNCTIONS:
    	n/a

Nintendo® Confidential Warning: all information in this document is confidential and covered by a non-disclosure agreement. You are responsible for keeping this information confidential and protected. Nintendo will vigorously enforce this responsibility.
Copyright © 1998
Nintendo of America Inc. All rights reserved
Nintendo and N64 are registered trademarks of Nintendo
Last updated March 1998