# mfsRomGetDestination
mfsRamGetDestination

    Format:	s32 mfsRomGetDestination(void)
    	s32 mfsRamGetDestination(void)
    Arguments:	None
    Return value:Destination code (a negative value is an error)
    Function:	Obtains destination code
    Description:	This function obtains the destination code.
    The destination codes are as follows.

    	MFS_DESTINATION_JAPAN	0	Japan-oriented
    	MFS_DESTINATION_US	1	US-oriented

    Main errors:
    	MFS_ERR_NOTMFSDISK Not an MFS-format disk
                              The disk ID's disk use is not 1, or the header is different.
    	MFS_ERR_VERSION	Different version disk