Function name:mfsSetRtc 芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋 Format: s32 mfsWrtieRTC(LEODiskTime* time) Arguments: time LEODiskTime structure buffer Return value: Error Function: Sets internal RTC Description: This function sets the date and time of the internal RTC to the values specified by time. It enables LeoSetRTC to be handled by using the MFS library. Main errors: MFS_ERR_NO Normal termination MFS_ERR_DEVICE Device error An error occurred in an internally called Leo function. Since a Leo function error is stored in the variable mfsError, check this variable to perform processing.