Function name:mfsSetLeoReadyFunc 芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋芋 Format: void mfsSetLeoReadyFunc(void (*func)(void)) Arguments: func Return value: None Function: Registers PI control function (after using PI) Description: This function registers a callback function that is to be called within MFS after an asynchronous Leo function is called. The callback function registered by this function mainly includes PI exclusive control code.