N64® Functions Menu

al - Audio Library Functions
gDP - DP GBI Macros
gdSP - General GBI Macros
gSP - SP GBI Macros
gt - Turbo Microcode RDP
gu - Graphics Utilities
Math - Math Functions
nuSys - NuSystem
os - N64 Operating System
sp - Sprite Library Functions
uh - Host to Target IO
64DD - N64 Disk Drive

Nintendo® Confidential

## osDpSetStatus

Syntax

#include <ultra64.h>
void osDpSetStatus(u32 status);
Explanation
The osDpGetStatus, osDpSetStatus, and osDpSetNextBuffer functions control and interrogate the display processor (DP). In other words, they provide basic control for the DP interface.
The osDpSetStatus call updates the DP command status register with status. The bits of potential interest include:

- DPC_CLR_TMEM_CTR - Reset DP TMEM counter.
- DPC_CLR_PIPE_CTR - Reset DP PIPE counter.
- DPC_CLR_CMD_CTR - Reset DP CMD counter.
- DPC_CLR_CLOCK_CTR - Reset DP CLOCK counter.

See Also
osDpGetStatus
osDpSetNextBuffer
osDpGetCounters

Nintendo® Confidential Warning: all information in this document is confidential and covered by a non-disclosure agreement. You are responsible for keeping this information confidential and protected. Nintendo will vigorously enforce this responsibility.
Copyright © 1998
Nintendo of America Inc. All rights reserved
Nintendo and N64 are registered trademarks of Nintendo
Last updated March 1998