# mfsHGetVolumeRC

Format: s32 mfsHGetVolumeRC(s32 drive)

Arguments:

drive Drive name ('A', 'B', ...)

Return value:Update counter value (a negative value is an error)

Function: Obtains update counter of volume

Description: This function obtains and returns the update counter of the drive specified by drive. Since the update counter only exists in the RAM area, the MFS_ERR_REFUSE error will occur if this function is used for the ROM area.

Main errors:

    MFS_ERR_NOTFOUND	Drive not found
    MFS_ERR_REFUSE		Illegal operation